    The Project Gutenberg EBook of Hand Grenades, by Graham M. Ainslie

    This eBook is for the use of anyone anywhere in the United States and most
    other parts of the world at no cost and with almost no restrictions
    whatsoever.  You may copy it, give it away or re-use it under the terms of
    the Project Gutenberg License included with this eBook or online at
    www.gutenberg.org.  If you are not located in the United States, you'll have
    to check the laws of the country where you are located before using this ebook.

    Title: Hand Grenades
           A handbook on rifle and hand grenades

    Author: Graham M. Ainslie

    Release Date: February 25, 2018 [EBook #56638]

    Language: English

    Character set encoding: UTF-8

    *** START OF THIS PROJECT GUTENBERG EBOOK HAND GRENADES ***

    Produced by Chris Curnow, Paul Marshall and the Online
    Distributed Proofreading Team at http://www.pgdp.net (This
    file was produced from images generously made available
    by The Internet Archive)

# HAND GRENADES

A HANDBOOK ON RIFLE
AND HAND GRENADES

COMPILED AND ILLUSTRATED BY

Major GRAHAM M. AINSLIE

FIRST EDITION

NEW YORK

JOHN WILEY & SONS, Inc.

London: CHAPMAN & HALL, Limited
1917

Copyright, 1917, by

GRAHAM M. AINSLIE

PRESS OF
BRAUNWORTH & CO.
BOOK MANUFACTURERS
BROOKLYN, N. Y.

[Pg iii]

PREFACE

The purpose of this work is to assist students of grenade work in acquiring a rapid and complete knowledge of the subject. If the student will refer constantly to the illustrations, which are accurate drawings of grenades now in use, this book may help to elucidate many points which are inadequately treated in any existing work.

In compiling the book, the author has inserted only information absolutely necessary, and has arranged it so simply that a person with a very little previous knowledge of the subject may be able to grasp both the data given, and the principles, and methods herein explained and illustrated.

This book is the result of practical experience in the present war.

G. M. Ainslie.

[Pg iv]

[Pg v]

CONTENTS

PAGE
Introduction | 1
Hand and Rifle Grenades | 2
Grenade Establishment | 26
Grenade Squad | 28
Clearing a Trench from a Flank | 29
Frontal Attack | 32
Trench Storming Parties | 36
Foreign Grenades. French | 38
Foreign Grenades. German | 42
Explosives used in Grenades | 51
Fuses, Detonators, etc. | 55
Throwing | 59

[Pg 1]

## HAND GRENADES

A grenade is a hollow ball, cylinder, or cube, made of metal or other material, which is filled with some explosive, and burst by means of a fuse, or on impact when it falls among an enemy. Until about the end of the seventeenth century trained soldiers called Grenadiers used grenades which were thrown by hand, but after that date they fell into disuse. In 1899—1900 at the siege of Mafeking they are said to have been used by the besieged, and also in the Russo-Japanese war. In the year 1914, however, the beginning of the great war produced new methods in the employment of infantry in the attack or defense of positions. It was proved that under many conditions infantry armed only with a rifle and bayonet found it impossible to press home an attack or hold a position against troops armed with grenades.

This weapon, handy to use and immensely destructive and demoralizing in its employment, has played a most important part in every successful operation carried out by British troops on the Western front. It has become one of the principal weapons not only in trench warfare, but in the attack and clearing of enemy positions, strong points, villages, and especially in house-to-house and cellar fighting.

Note. 1. In throwing all hand grenades an overarm action will be used, like a bowler when playing cricket.

2. Attached to all stick hand grenades are tapes or streamers a couple of feet long to enable them to fly head first, when thrown.

[Pg 2]

## BRITISH GRENADES

There are two kinds of grenades:

- No. 1. Time grenades.
- No. 2. Percussion grenades.

No. 1 rely for ignition upon:

- (a) Some form of fuse lighter.
- (b) A length of time or safety fuse.
- (c) A detonator or exploder.

No. 2 on:

- (a) Some form of percussion striking device.
- (b) A percussion cap.
- (c) A detonator.

For throwing purposes grenades as follows:

- 1. Hand grenades.
- 2. Stick hand grenades.
- 3. Rifle grenades, fitted with firing rods 8 to 10 in. long.

### GRENADE HAND NO. 1 or General Service

Type. Percussion stick grenade.

Weight. Two lb. complete.

Explosive. Lyddite.

Safety Device.

- 1. Safety pin. Leather thong through eye of pin.
- 2. Cord becket.
- 3. Red indicator and words of directions on removable cap.

[Pg 3]

Grenade Hand No. 1, Mark I.

[Pg 4]

Body. Brass cylinder.

Striker. Steel needle carried in removable cap.

Detonator. Special detonator (see page 57.)

To prepare for use:

- 1. Turn word “remove” on cap to red indicator.
- 2. Take off removable cap.
- 3. Insert detonator. Turn to left to secure.
- 4. Replace cap and turn to “travel.”

To fire:

- 1. Turn cap to “fire.”
- 2. Pull out leather thong from safety pin. Remove
- cord becket.
- 3. Gather streamers palm right hand, holding
- grenade in left hand.
- 4. Holding grenade right hand, pull out safety pin
- with left hand.
- 5. Throw grenade.

Packing: Grenades are packed six in wooden box with tin containing ten special detonators.

Precautions: Care must be taken in act of throwing that grenade does not strike any object in rear of the thrower.

Always carry grenades at “travel.”

### GRENADE HAND NO. 2

Hales Hand or Mexican Grenade

Type. Percussion stick grenade.

Weight. One lb. complete.

Explosive. Tonite.

Safety Device. Safety pin.

Body. Brass cylinder 4¾ × 1¼ in. diameter.

Striker. Brass needle pellet 1½ in. long, conical head, steel needle point, creep spring contained in brass base piece. [Pg 5]

Grenade Hand No. 2. Hales Grenade.

[Pg 6]

Detonator. Special No. 2.

To prepare for use:

- 1. Holding grenade head downwards, unscrew black
- ebonite, if needle pellet found secure.
- 2. Screw in detonator.

To fire:

- 1. Holding grenade in left hand, gather streamers
- palm of right hand.
- 2. Holding grenade right hand, pull out safety
- pin with left hand.
- 3. Throw grenade.

Packing. Grenades are packed ten in a wooden box, with tin containing ten No. 2 detonators.

Precautions. See Hand Grenade No. 1.

### “GRENADE 303.” SHORT RIFLE NO. 3

Hales Rifle Grenade

Type. Percussion.

Weight. One lb. 5 oz.

Explosive. Tonite.

Safety Device:

- 1. Safety pin.
- 2. Releasing collar.
- 3. Wind vane.
- 4. Retaining bolts.

Body. Serrated steel cylinder.

Striker. Brass fluted needle pellet 1½ in. long, wasp waisted, conical head, steel needle point and creep spring, contained in brass base piece.

Detonator. Special No. 3 (see p. 57.)

[Pg 7]

“Grenade 303.” Short Rifle No. 3, Mark I
(or Hales Rifle Grenade).

[Pg 8]

To prepare for use:

- 1. Holding grenade head downwards, unscrew black
- ebonite block, if needle pellet found secure.
- 2. Screw in detonator.

To fire:

- 1. Oil rod and barrel of rifle.
- 2. Insert rod into barrel of rifle and work it up and
- down to ensure lubrication and to expel air.
- 3. Place special cartridge in chamber rifle and close bolt.
- 4. Pull out safety pin.
- 5. Pull down releasing collar.
- 6. Give wind vane 1½ turns to left.
- 7. Fire the rifle.

Packing. Grenades packed twenty in wooden box in protecting tins with screw-off lids and four tins containing 20 in. special detonators, rifle, grenades and twenty-two special blank cartridges.

### GRENADE HAND NO. 5. MARK I.

Mills Hand Grenade

Type. Time 4½ seconds.

Weight. One and one-half lb.

Explosive. Ammonal.

Safety Device:

- 1. Safety pin.
- 2. Striker lever.

Body. Serrated oval cast-iron.

Striker. Steel rim firing. [Pg 9]

Igniter. Special, consisting of a separate unit. Special N.g. cap holder, N.G. rim firing percussion cap, 1¾ in. safety fuse and detonator.

To prepare for use:

- 1. Unscrew base plug.
- 2. Examine detonator and striker well for faults.
- 3. Insert special igniter.
- 4. Screw on base plug tightly by means of special key.

Grenade Hand No. 5, Mark I (or Mills Grenade).

[Pg 10]

To fire:

- 1. Hold grenade in right hand, base plug up, the
- fingers holding the striker lever firmly against
- the body of the grenade, the ring of the safety pin
- towards the left hand.
- 2. Pull out safety pin with the left hand, keeping
- the pressure on the striker lever.
- 3. Throw the grenade.

Packing. Grenades are packed twelve in wood box, with a tin containing twelve igniters.

Mills Rifle Grenade

Base plugs into which are screwed 8 in. rods are provided for this grenade to be fired from rifle, a special one being fitted to the rifle for this purpose.

### GRENADES HAND NOS. 6 AND 7

R.L. or T.G. Grenades

Type. Time and friction.

Weight. No. 6 or light grenade, 1 lb. complete; No. 7, or heavy grenade, 1 lb. 13 oz.

Explosive.

Safety Device. Papier maché cap.

Body. Tin cylinder with rounded ends 4 in. long, 2¼ in. diameter.

Igniter. Special friction igniter, length of safety fuse, and service detonator combined.

To prepare for use:

- 1. Take off papier maché cap.
- 2. Take wooden plug out of detonator tube.
- 3. Insert friction lighter, turn to left and lock,
- clipping flange under studs.
- 4. Replace papier maché cap.

[Pg 11]

To fire:

- 1. Remove papier maché cap.
- 2. Hold grenade right hand, becket towards the wrist.
- 3. Pull out becket sharply with left hand.
- 4. Throw grenade at once.

Grenade No. 6, Mark I.

[Pg 12] Packing. Grenades packed forty in wooden box. Four haversacks with four tins containing ten special igniters. These grenades should always be carried with papier maché caps on.

Note. The No. 6 grenade is an assault or demoralizing grenade.

### GRENADE HAND NOS. 8 AND 9

Double Cylinder

Type. Time.

Weight. No. 8 light pattern, 1 lb. 6 oz. complete; No. 9, heavy pattern, 2 lb. complete.

Explosive.

Safety Device.

Body. Tin cylinder 2¾ × 1½ in. diameter, inside larger cylinder 3¼ × 3 in. diameter.

Igniter. Special Nobel lighter 1¾ in. safety fuse No. 8, VII detonator.

Grenade No. 8.

[Pg 13] To prepare for use:

- 1. Crimp lighter on to fuse, insert fuse into detonator
- and crimp the latter on to fuse. Wax joints at
- lighter and detonator.
- 2. Insert igniter into detonator tube in inner
- cylinder.
- 3. Wax round joint where igniter enters grenade.
- 4. Wire fuse on to grenade.

To fire:

- 1. Hold grenade right hand, gripping bottom of
- Nobel lighter between thumb and finger.
- 2. Tear off tape and pull out safety pin.
- 3. Press down outer tube of N. lighter, turn sharply
- to R. or L.
- 4. Throw grenade at once.

Note. The heavy pattern grenade has more shrapnel and less explosive than the light pattern grenade.

### GRENADE HAND NO. 12

Hairbrush or Box Pattern Grenade

Type. Time, or land mine.

Weight. Three lb. complete.

Explosive. Ammonal or guncotton.

Safety Device. Safety pin.

Body. Tin box 3×5×2 in. A grooved cast-iron plate, ¼ in., forms the front side.

Igniter. Special brass tube consisting of spring and striker held in place by safety pin. Cap and fuse and detonator or Nobel lighter, fuse and detonator.

To prepare for use. See Nos. 8 and 9 grenades.

To fire. See Nos. 8 and 9 grenades.

Note. This grenade is now used as a land mine.

[Pg 14]

Grenade No. 12.

[Pg 15]

### BATTYE GRENADE

Type. Time.

Weight. One lb. 2 oz. complete.

Explosive. Ammonal guncotton, 1½ oz.

Safety Device. Safety pin in Nobel lighter.

Body. Cast-iron cylinder, 3 × 2 in. diameter, one end solid.

Igniter. Nobel lighter, 1¾ in. fuse, No. 8 M.K. VII detonator.

To prepare for use. See Grenade Hand No. 8.

To fire. See Grenade Hand No. 8.

Packing. Grenades packed thirty in wooden box arranged with removable wooden partitions which rest on top of the grenades, to prevent lid coming in contact with the end of the igniters.

Battye Hand Grenade.

[Pg 16]

### PITCHER HAND GRENADE

Type. Time.

Weight. One and one-half lb.

Explosive. Ammonal.

Safety Device.

Body. Cast-iron cylinder 4 × 1⅞ in. diameter, one end solid.

Igniter. Special.

This grenade is not likely to be reissued. The igniter is described in the Training and Employment of Grenadiers issued by General H. Q., October, 1915.

Pitcher Hand Grenade.

[Pg 17]

### OVAL GRENADE

Type. Time.

Weight. One lb. 2 oz. complete.

Explosive. Ammonal.

Safety Device. Brock lighter. (See Patent Lighters, p. 58.)

Body. 3⁄16 in. cast-iron, egg-shaped, 3½ in. long × 2¼ in. diameter at middle.

Igniter. Brock lighter, 1¾ in. fuse, No. 8 M.K. VII detonator.

To prepare for use. See Hand Grenade No. 8.

To fire:

- 1. Hold grenade right hand.
- 2. Pull off waterproof paper on Brock lighter with
- left hand.
- 3. Strike lighter against brassard carried on left
- arm for this purpose.
- 4. Throw grenade at once.

Precautions. The waterproof paper must not be removed before throwing, as composition may get damp, or grenade accidentally lighted.

### BALL GRENADE

Type. Time.

Weight. One lb. 11½ oz. complete.

Explosive. Ammonal, 5½ oz.

Safety Device. Safety pin in Nobel lighter. (See Patent Lighter.)

Body. Cast-iron sphere, 3 in. diameter.

Igniter. Nobel lighter, 1¾ in. fuse, No. 8 M.K. VII detonator. [Pg 18]

To Prepare for Use. See Hand Grenade No. 8.

To Fire. See Hand Grenade No. 8.

Ball Grenade.

### NEWTON HAND GRENADE

Type. Time, 4½ seconds.

Weight. One lb. 5 oz.

Explosive. Ammonal.

Safety Device. Special split tin disc over N.G. percussion cap.

Body. Cast-iron, pear-shaped.

Striker. Contained in special striker cap.

Igniter. Sawed off .303 in. blank cartridge, 1½ in. safety fuse, detonator.

To Prepare for Use:

- 1. Remove striker cap.
- 2. Insert igniter.
- 3. Slip on safety device.
- 4. Replace striker cap.

[Pg 19]

Newton Hand Grenade.

[Pg 20]

To Fire:

- 1. Hold grenade in right hand, narrow end downwards.
- 2. Bring striker cap down a sharp blow on brassard
- carried on left thigh for that purpose, or upon
- some hard surface.
- 3. Throw grenade at once.

### NEWTON RIFLE GRENADE

Type. Percussion.

Weight. One lb.

Explosive. Ammonal.

Safety Device. Newton Hand.

Body. Cast-iron conical.

Striker. Newton Hand.

Detonator. Commercial.

To Prepare for Use:

- 1. Remove striker cap.
- 2. Insert detonator.
- 3. Slip on safety device.
- 4. Replace striker cap.

To Fire:

- 1. Oil 10 in. rod and barrel of rifle.
- 2. Work rod up and down to insure lubrication
- and to expel air.
- 3. Place special blank cartridge in chamber of
- rifle and close bolt.
- 4. Fire the rifle.

[Pg 21]

Newton Rifle Grenade.

[Pg 22]

### HAND GRENADE NO. 19

Type. Percussion stick grenade.

Weight. One and three-quarter lb.

Explosive. Ammonal.

Safety Device:

- 1. Safety pin.
- 2. Shearing wire.

Body. Oval, cast-iron.

Striker. Mushroom-topped brass.

Detonator. Special long commercial.

Igniter. (Sawed off) 380 in. blank cartridge.

To Prepare for Use:

- 1. Unscrew brass striker holder.
- 2. Insert detonator.
- 3. Screw on brass striker holder.

To Fire:

- 1. Unwind streamer at end of handle.
- 2. Hold grenade in left hand, gather up streamers
- palm of right hand.
- 3. Holding grenade in right hand, take out safety
- pin with left hand.
- 4. Throw grenade.

Packing. Grenades are packed twelve in a wooden box, also a tin containing twelve special detonators.

[Pg 23]

Grenade No. 19. Hand.

[Pg 24]

### RIFLE GRENADE NO. 20

Improved Hales Rifle Grenade

Type. Percussion.

Weight. One lb. 8 oz.

Explosive. Tonite.

Safety Device:

- 1. Safety pin.
- 2. Releasing collar.
- 3. Retaining bolts.

Body. Steel cylinder.

Striker. Same as No. 3 Rifle Grenade (see p. 7).

Detonator. Special No. 3 (see p. 7.)

To Prepare for Use:
1 and 2. See No 3 Rifle Grenade (see p. 7).

To Fire:
1, 2, 3, and 4 same as No. 3 rifle grenade,
see p. 7, Fire Rifle.

Packing. Grenades packed twenty in wooden box, four tins containing five each “special detonators rifle grenade,” and 22 special blank cartridges.

Precautions. See all stick hand grenades.

[Pg 25]

Rifle Grenade No. 20.

[Pg 26]

## DIVISIONAL GRENADE ESTABLISHMENT
AND CHAINS OF AUTHORITY

Divisional Grenade Officer and Instructional Staff for Grenade, Stokes Gun, Trench Mortar Schools.

Brigade Grenadiers:

- 1. Sergt. Major.
- 1. Q.M.S.
- 4. Sergt. Instructors.
- 4. Grenade platoons, per battalion in brigade.

Battalion Grenadiers of Grenade Platoon:

- 1. Grenade officer.
- 1. Sergt. Instructor.
- 4. N.C.O.’s and 40 men.
- 1. Cook.
- 1. Officers’ servant.

Total, 48 all ranks.

Company Grenadiers:

- 1. N.C.O. and 10 men per platoon.
- 4. N.C.O.’s and 40 men per company.
- 16. N.C.O.’s and 160 men per battalion.

Total grenadiers per battalion, 224 all ranks.

Total grenadiers per brigade, 896 company and battalion grenadiers.

Total grenadiers per division, 2688 company and battalion grenadiers. [Pg 27]

Divisional Grenadier Establishment Showing Chain of Responsibility.

[Pg 28]

## COMPOSITION OF A GRENADE SQUAD

In Line

- No. 1. Bayonet man.
- No. 2. Bayonet man.
- No. 3. First thrower.
- No. 4. Second thrower.
- No. 5. N.C.O. or Leader.
- No. 6. First carrier.
- No. 7. Second carrier.
- No. 8. Spare man.
- No. 9. Spare man or sniper.

In Single File

- No. 1. Bayonet man.
- No. 2. Bayonet man.
- No. 3. First thrower.
- No. 6. First carrier.
- No. 5. N.C.O. or Leader.
- No. 4. Second thrower.
- No. 7. Second carrier.
- No. 8. Spare man.
- No. 9. Spare man or sniper.

Duties of Above. Nos. 1 and 2 Bayonet Man.

1. Clearing of a Trench to a Flank. They are the bodyguard for the thrower and carrier and must always protect them under any conditions and at all costs.

Note. The latter are not armed against attack at close quarters. The bayonet men work in advance of the thrower and carrier of their squads. They act as trench scouts; that is, they instruct their thrower and carrier how the trench runs and where the dug-outs and side trenches will be met. They will carry their rifles with bayonets fixed, loaded, magazine full. No. 3 and 6 bomb and clear all dug-outs on the way down the trench. The first man throws the bomb, the bayonet man enters the dug-out and completes its work. At the junctions of communication trenches and side trenches they act as trench sentries and observers until relieved by the squads in rear. If necessity arises they assist the thrower by throwing bombs.

2. Frontal Attack against Enemy Positions. They will be in line with, not in advance of the thrower and carrier and will protect them while throwing by snap shooting, or with their bayonets against assault, or a sudden rush by the enemy when at close quarters.

[Pg 29]

Clearing a Trench from a Flank.

[Pg 30]

3. Street Fighting and Village Cleaning. They will keep down enemy rifle fire by snap shooting, so as to enable the thrower to work close enough to his objective to throw grenades, and when these have burst, will go forward and complete their work.

No. 3. First Thrower. He throws grenades according to the directions given him by his leader or by his bayonet men. He is a picked man, steady under fire and chosen for his accuracy and length in throwing.

No. 4. The Carrier. He follows close enough in rear of the throwers to keep them supplied with grenades, but must be careful not to crowd them or impede the throwing. He will be prepared to instantly take up the duties of the thrower should he become a casualty.

No. 5. N.C.O. or Leader. He is responsible for his squad and the proper carrying out of the duties given to the squad. He will inspect each man before an attack and see that he has his complete equipment and that he knows the general idea and direction of the attack and the final objective of his squad. He will be responsible for the maintenance of supplies of grenades through his squad to the thrower, and will supervise the automatic filling up of casualties in his squad by men from the squads in the rear. He will indicate the position and progress of his squad in the attack to supporting troops, etc., by means of flags or other signals by day and by colored flares by night.

Nos. 6, 7, 8 and 9. Their duties are the same as Nos. 1, 2, 3 and 4, and are to be considered primarily as carriers until otherwise employed. [Pg 31]

No. 10. Spare Man. He will act, if necessity arises, as leader of his section, to clear side trenches, etc., and will instantly take over the duties of No. 5 should he become a casualty.

No. 11. Sniper. He will act as a sniper by day and a connecting file by night, between his own squad and the squad of troops in rear.

Note. Every man in the grenade squad should be trained to fill the position of any other in the squad.

Explanation of Chart No. A2. The position occupied by grenadiers in an attacking squad has this main point in consideration.

The safety and local protection of each individual in the squad; care should be taken that as far as possible each man has a solid corner of the trench close to him, which he can use as a protection against the bursting effect of enemy grenades, by quickly advancing or retiring around the corner.

The bayonet men are in advance of the thrower, close enough to protect him, and not too far in front as to be in danger of being bombed by him.

The thrower—the actual means of attack—is protected in front by the traverse and in the rear by the corner of the parados. The carrier is close behind the thrower and is protected by two corners. The N.C.O. or leader is where he can best watch the flight of the grenades thrown by the throwers, and is also equally well protected.

Method of Advance. It is usually the endeavor to bomb and clear three bays at a time in advance of the bayonet men. The N.C.O. reports the throwing by the word “Mark,” to indicate a burst in the required bay. On the third mark having been registered, the N.C.O. gives the order, “Bayonet men report.” They immediately advance up the trench to the last bay cleared and report back after examination either “All [Pg 32] clear” or “Enemy holding,” whereupon the N.C.O. gives the order “Advance,” or directs the thrower to bomb the last bay again. This means of advance is continued until the objective is gained.

Island Traverse. The two methods of attack are employed as shown on the chart. It is imperative that the attack must not be allowed to be held up, and should it be found impossible to advance down the trench itself, owing to enfilade fire, the attack must be immediately launched outside the trench, so as to attack the traverse from the rear, in the case of a daylight attack.

Precautions. Care must be taken, especially by the bayonet men in their advance through the trench, that enemy concealed trenches, dug-outs, etc., are not left undiscovered. The sides of trenches and the walls and floors of dug-outs should be carefully examined for concealed entrances or exits.

## FRONTAL ATTACK

In Conjunction with Infantry

The Preparation Before an Attack. The following details must be carefully considered:

(a) The study of operation orders.

(b) The linking up of observations gained from the

- 1. Study of existing trenches and aeroplane maps
- of enemy positions.
- 2. The personal reconnaissance of the topographical
- features of the ground to be covered in the advance.

(c) The detailing of squads to their special objectives and the arranging for work, carrying wire and demolishing parties for permanent blocks at the final objectives.

[Pg 33]

Frontal Attack.

[Pg 34]

(d) The kind of grenades to be used with a view to facilitating the carrying of same.

(e) Carrying parties must be told off to insure supplies of grenades reaching the throwers.

(f) Grenade depots must be built, sign boards arranged for, and clearly marked “Grenade Depot” not only in our own system of trenches, but also the positions told off beforehand where they are to be established in the enemy trenches, or in No Man’s Land immediately previous to the attack.

(g) Responsible officers and N.C.O.’s should be told off to look after the grenade depots and supply of grenades.

(h) The position for infantry grenade dumps must be selected and clearly explained to all units taking part in the attack, and special parties told off to collect at these points and carry grenades to nearest depots.

(i) A traffic system should be arranged and all men must be acquainted with it, and the trenches or lines of travel clearly marked “up traffic,” etc.

The Advance.

- 1. In line with infantry.
- 2. In advance of infantry.

No. 1 is the method adopted in daylight attack, the advance not being covered by gas or smoke clouds.

No. 2 is method adopted in night attack and when weather conditions or topographical features of ground covered in the advance allow it.

Attacking squads are allotted positions in lines of infantry immediately opposite their first objectives, and on reaching these positions should immediately commence bombing and clearing the trenches towards their final objectives. In the case of No. 1 the infantry clears [Pg 35] the main trench, but special grenade parties may be told off to assist the infantry in this work, especially when strong points occur in the enemy position.

It is most important that all infantry taking part in an attack should be previously supplied with grenades and this must be considered the first source of supply. Positions designated as infantry grenade dumping positions should be chosen and known to the infantry at which they dump their grenades in their advance on the enemy positions. These positions should be close to the position to be captured and held.

In order to hold positions captured from the enemy it is imperative that grenade storming parties hold their final objectives at all costs, and until the positions to be permanently held have been consolidated.

[Pg 36]

## TRENCH STORMING PARTIES

Trench storming parties should kill or drive back the hostile occupants of a trench as quickly as possible, clear as much of the enemy trench as has been ordered, and then hold the portion cleared with as small loss as possible to themselves. It must be remembered that in trench clearing, and especially in deep and narrow trenches, only the head of the attacking party can directly kill, and seldom more than one man can throw at a time. Therefore it is essential that a constant supply of grenades reaches the thrower and that the places of casualties are automatically filled by reinforcements. Men must be trained until they can do this either by day or at night time.

Advance. Movement is rapid until contact with the enemy is obtained. Once contact is established it must be maintained and pressed home. A retreating enemy must be given no time to re-establish a defensive attitude, corners must be worked carefully and bays and straight pieces of trench rushed. The bayonet men will complete the work of the grenades and see that the carrier and thrower will meet with no opposition on their way to new throwing position. The effect of a grenade bursting in a confined space like a trench is tremendous, and though it may not kill it will stun or shock the hostile occupants, and if the bayonet men follow up rapidly they will meet with very little resistance.

Casualties. Every man must be trained to take up the duties of any other man in his squad. They do not necessarily keep to their own [Pg 37] squads; the squads in rear of the attacking squad may be looked on as a reserve squad for the one in front. Thus, Casualty first squad. The thrower No. 3 is reinforced by the first thrower of the second squad, and so on.

Side Trenches. When a side trench is met with, the leading squad will go up and clear it. The second half will remain at the junction until first returns, then the second squad will continue advance in original direction of the attack.

Blocking and Barricades. For blocking captured trenches, etc., see Manual of Field Engineering, Wire Entanglements, Hurdles, etc.

[Pg 38]

## FOREIGN GRENADES. FRENCH

The description of British and German grenades apply also to those grenades used by the French army. They are:

- 1. Three kinds of petards.
- 2. Pear-shaped percussion grenade hand.
- 3. The “Besozzi” grenade.

Ball Grenade.

### 1. BALL GRENADE OR FORTRESS GRENADE

Description

Igniter. Friction tube with wire pull let into wooden fuse.

Safety Devices:

- 1. The fuse is carried separate.
- 2. The plug is covered with paper.
- 3. The wire pull is bent to prevent a direct pull of the fuse.

To Use. See German spherical Grenade, p. 43. [Pg 39]

### 2. PEAR-SHAPED GRENADE—Percussion

Description

Igniter. A copper tube containing striker, creep spring and detonator.

Pear-shaped Grenade.

Safety Devices:

- 1. The cams lever secures striker while the lever
- is held in place against body of grenade.
- 2. The strong loop which holds lever against body
- of grenade and is fastened by a metal seal.

[Pg 40] How to Use;

- 1. This grenade is always “alive.”
- 2. Holding grenade in right hand, neck towards the
- wrist, the lever against the palm of the hand.
- 3. Pull off the metal seal with left hand.
- 4. Throw the grenade.

Note. This grenade must be carefully handled; it is carried and packed “alive.”

Besozzi Grenade.

### 3. BESOZZI GRENADE

Description

Igniter:

- 1. Time fuse which projects from the grenade.
- 2. Red phosphorus tipping to fuse.
- 3. Detonator.

Safety Devices:
1. The grenades are packed in waterproof paper.

[Pg 41] To Use:

- 1. Holding grenade in the right hand, fuse upwards.
- 2. Strike the phosphorus tip with a downwards
- motion of the left hand, with the striking box.
- 3. Throw the grenade at once.

Notes. 1. Fuse burns 5 seconds.
2. These grenades are always carried alive.
3. A special ring or striking box is provided to light the fuse.

Foreign Hair Brush Grenades. They are similar to the British No. 12 Hand Grenades.

[Pg 42]

## GERMAN GRENADES

There are two types:

- No. 1. Service grenades.
- No. 2. Improvised or home-made grenades.

These are again divided into two classes:

A. Those that depend for their effect upon fragmentation on detonation.

B. Those that depend for their effect upon the shock of detonation only.

The type B is more commonly met with than type A. Ignition is by time or percussion. The time of fuses about six seconds burning.

Precautions. When handling foreign grenades care should always be taken and the following rules should be enforced:

- 1. Only skilled grenadiers should be allowed to examine
- and handle any grenades found.
- 2. Grenade depots when discovered should be immediately
- reported to the nearest grenadier.
- 3. Foreign time grenades should be thrown as soon
- as the lighting device has been started.

Description of German Grenades

As the means of firing a grenade will be immediately apparent to the skilled grenadier on seeing the grenade, the following information only is of importance to the unskilled grenadier:

- 1. How to make the grenade safe.
- 2. How to make the grenade alive.
- 3. How to use the grenade against the enemy.

[Pg 43]

### SPHERICAL GRENADE

1. How to Make Safe:

1. Screw out the special lighter, taking care not to pull the wire.

2. How to Make the Grenade Alive:

- 1. Screw in the special lighter.
- 2. Remove the oiled paper, straighten the wire.

3. How to Use the Grenade:

- 1. Put on wrist strap.
- 2. Hold grenade in the right hand, igniter towards
- the wrist.
- 3. Hook the swivel of the wrist strap on to the
- wire pull of the grenade.
- 4. Throw the grenade at once.

Note. Use time of fuse burning, seven seconds, but another lighter which burns for five seconds—painted red—is also provided.

### STICK CYLINDER GRENADE

See p. 44.

1. How to Make Safe:

- 1. Remove the handle and base plug by raising
- turned down edge of the cylinder carefully.
- 2. Empty contents of cylinder.

2. How to Make the Grenade Alive:

1. See the British Grenades Hand No. 12.

3. How to Use the Grenade:

- 1. Pull out safety pin.
- 2. Throw the grenade at once.

Note. Fuse about 2 in. long. Burns about six seconds.

[Pg 44]

Stick Cylinder Grenade.

### SMALL STICK CYLINDER GRENADE

See p. 45.

1. How to Make Safe:

1. Take out igniter.

2. How to Make the Grenade Alive:

- 1. Take out wooden plug and insert the igniter.
- 2. Tear off paper cover from the lighter.

3. How to Use the Grenade:

- 1. Holding grenade in right hand, rub the match
- head on the side of a match box, etc.
- 2. Throw the grenade at once.

Note. Time fuse burns about six seconds.

[Pg 45]

[Pg 46]

### CYLINDRICAL GRENADE

See p. 44.

Regulation Type

1. How to Make Safe:

- 1. Unfasten clips which hold lid of cylinder.
- 2. Remove cardboard cylinder containing explosive.
- 3. Insert hand and withdraw detonator from brass
- tube at end of handle.

2. How to Make Alive:

- 1. If drawing loop is attached to handle by paper
- band, unscrew handle and insert special detonator
- into brass tube at end of handle and refix handle.

3. How to Use the Grenade:

- 1. Holding grenade in right hand.
- 2. Pull loop sharply with left hand.
- 3. Throw the grenade at once.

Note. Time fuse burns is stamped on handle 5½ or seven seconds. Care must be taken when grenade is found without the pull loop, in case it has been fixed to light on unscrewing handle.

### OYSTER SHELL OR DISC HAND GRENADE

See p. 47.

1. How to Make Safe:

- 1. If safety pin is in place, unscrew cap marked S.
- 2. Remove detonator.

Note. If safety pins and safety tubes are not in place, the above must be done without disturbing the grenade.

2. How to Make Alive:

1. This grenade is packed alive.

3. How to Use the Grenade:

- 1. Holding grenade in right hand, safety pin upwards,
- pull out safety pin with left hand.
- 2. Pull off the cap of the safety tube.
- 3. Holding the grenade with the first or middle
- finger on top of the safety tube and the ball
- of the thumb over the cap marked B.
- 4. Throw the grenade with its edge vertical.

Note. A low or horizontal throw may cause a failure.

[Pg 47]

Disk Hand Grenade.

### PARACHUTE GRENADE

See p. 48.

1. How to Make Safe:

- 1. Unscrew the plug in the head.
- 2. Withdraw the detonator.

2. How to Make Alive:

- 1. Unscrew the plug and insert detonator, fulminate
- downwards.
- 2. Screw the plug and tear off band holding parachute.

[Pg 48]

Parachute Grenade.

3. How to Use the Grenade: [Pg 49]

- 1. Hold loop of cord firmly with fingers of right hand.
- 2. Tear out plug from handle and unwind a short
- length of the cord.
- 3. Holding the grenade in right hand, the first and
- second fingers firmly in the loop of the cord.
- 4. Throw the grenade to a height of at least 3 to 4 yards.

Note. This grenade requires considerable practice.

### RIFLE GRENADES

See p. 50.

1913 and 1914

1. How to Make Safe:

- 1. Unscrew igniter plug in the head of 1913 grenade.
- Unscrew fuse from the body of 1914 grenade.

2. How to Make Alive:

- 1. Screw igniter into head of 1913 grenade.
- Screw fuse into body of 1914 grenade.

3. How to Use the Grenade:

1. Follow out custom of firing British Rifle Grenades.

Note. Only a German rifle can be used, and more care in handling the grenade before firing must be taken than with the British grenades, they are liable to become “alive” if dropped on to the tail rods.

[Pg 50]

Rifle Grenades.

[Pg 51]

## EXPLOSIVES USED IN GRENADES

Explosives are divided into two classes:

- 1. Low explosives.
- 2. High explosives.

To the first group belong all propellant explosives, i.e., all powders, such as gunpowder and smokeless powders used in firearms.

To the second group belong:

- (a) All explosives used in shells, torpedoes, grenades,
- demolitions, etc.
- (b) Detonators or exploders, i.e., explosives which start
- explosive reactions in the explosives of Group (a).

The characteristic of H.E. is the extreme violence and suddenness of their detonation.

In order to make them instantly pass from a solid or liquid form to gas, they require a detonator or exploder, which applies a violent shock to them and breaks down the chemical structure of the explosive compound, and enables the flame to pass instantaneously throughout the mass of the compound. This explosive is known as detonation.

The composition of H.E. almost without exception is some organic substance, usually some form of carbon combined with nitrogen. Nitrogen, one of the most inert gases known, owes its explosive value to this very inertness; it combines so very reluctantly that on the least provocation—such as shock—the compound of which it forms a part instantly breaks up into gas, giving the enormous expansion needed for explosive effect. [Pg 52]

Ammonal. A gray powder. An Austrian explosive, picric acid plus T.N.T. plus aluminum powder plus nitrate of ammonia plus carbon.

A very safe explosive—will not detonate when struck by rifle bullet, but is very hygroscopic (collects moisture) and when in this condition is liable not to detonate.

Ballistite. Consists of guncotton plus camphor or vaseline. Invented by Nobel in 1888.

Cordite. Consists of nitro-glycerine 55 parts, plus guncotton 37 parts, plus vaseline 5 parts, plus acetone to harden, invented by Sir W. Abel.

Benzol. Or Benzine, used extensively as a motor fuel contains a fair percentage of toluene. (See T.N.T.)

Coal Tar. When subjected to fractional and low-temperature distillation produces many by-products valuable in the making of H.E. These distillations give off “light” and “heavy” oils of coal tar.

Donnerite. High explosive employed by German army in grenades.

Dynamite. See Nitro-glycerine.

Fulminate of Mercury. See Mercury.

Guncotton, or nitro-cellulose consists of cotton waste, purified, dried, and heated with mixture of concentrated nitric and sulphuric acid. Washed and reduced to a pulp and moulded into 1 oz. primers and 15 oz. slabs for service use. Is considered inferior to lyddite.

- Size of wet slab of G.C., 6 × 3 × 1⅜ in.
- Wet guncotton will not explode if hit by a bullet.
- Wet guncotton can be sawn by a wet saw.
- Requires dry primer, detonator and fuse to explode.
- Dry guncotton will explode if hit by a bullet.
- Dry primer of guncotton 1.35 in. diam., 1.15 in. diam. at ends, and 1.25 in. high.
- Strength, 2½ times stronger than gunpowder, unconfined.
- Strength, 7 to 8 times stronger than gunpowder, confined.
- Invented by Schombein in 1846.

[Pg 53] Gunpowder. A mechanical mixture.

Saltpeter 75 per cent, plus charcoal 15 per cent, plus sulphur 10 per cent. Rate of burning depends upon firmness of powder.

Lyddite, or picric acid. Consists of melted and solidified picric acid. Vaseline is used to melt it. (See Picric Acid.)

Mercury Fulminate. Is made by dissolving three parts mercury in 36 parts nitric acid, keeping mixture at low temperature, and when dissolved adding 17 parts of alcohol.

A small quantity of F. of M. placed on top of T.N.T. forms an excellent detonating mixture. A great many German detonators consist of this. Discovered by Howard in 1800.

Melinite. A French H.E., very similar to lyddite. Is picric acid mixed with collodion. Introduced by Eugene Turpin.

Nitro-glycerine. Is produced by the action of nitric acid and sulphuric acid on glycerine. Invented in 1847. When pure is a colorless liquid. Explodes when heated to about 360° F.

N.G. in liquid form too dangerous to be used in practice. Was absorbed in porous solid by Nobel in 1867 as dynamite. Porous solid used either kiesulguhr or fullers’ earth used in percussion caps.

Relative strength | 150 equals maximum
Blasting glycerine | 150
Gelatine dynamite | 130
Gelignite | 110
Dynamite | 100
Carbonite | 55

Picric acid. A yellow crystalline prepared from coal tar. A by-product of gas manufacture. The “heavy oil” of coal tar is boiled [Pg 54] and chemically treated, resulting in phenol or carbolic acid, which separates from it. Carbolic acid is boiled sulphuric acid, and nitric acid is carefully added, resulting in picric acid.

It is a very safe explosive and very powerful. Its chief fault is that it forms “picrates” with metals or acid salts, some of which are more sensitive to disturbing influences than the acid itself. To overcome this the inside of all shells are varnished.

Pressure of picric acid equals 135,820 lb. on the square inch.

Shimose. Japanese H.E. Similar to lyddite.

T.N.T., or tri-nitro-toluene or Toluol, largely used in German army and navy. Is produced by heating toluene with mixture of nitric and sulphuric acid.

Less powerful than lyddite, but is more stable and does not form “picrates” and is not affected by water or air. Will not explode if hit by a bullet.

Pressure T.N.T. equal to 119,000 lbs. per square inch.

Tolite. French name for T.N.T.

Trilite. Spanish name for T.N.T.

Trotyl. German name for T.N.T.

Toluene, or Toluol. Experiments made in 1899 at Karlsruhe produced about seven pints of toluene from one ton of coal. The modern process of low-temperature distillation of coal, however, greatly increases quantity that can be obtained from each ton.

Is an aromatic colorless liquid hydrocarbon.

Turpinite. French H.E. similar to Melinite.

Tetryl. A coal tar product containing more nitrogen than T.N.T. or lyddite. When mixed with a lead oxide it makes a less sensitive and safer preparation than fulminate of mercury for detonators.

[Pg 55]

## FUSES

### SERVICE FUSE

No. 11 Safety or Time Fuse

Description. Color, black. Smooth surface.

Time of Burning. One foot in thirty seconds.

Composition. Train of slow match inside a wrapping of hemp or flax, covered by layer of gutta-percha, surrounded by binding of black waterproof tape.

### INSTANTANEOUS OR QUICK FUSE

Color, red. Ribbed surface.

Time of Burning. Eighty feet per second.

Composition. Same as service fuse, except that it contains quick match in place of slow match.

Caution. Instantaneous fuse must never be stored alongside safety fuse. [Pg 56]

### DETONATORS

SERVICE

No. 8 Mark VII

Description. Copper tube open at one end painted red, marked on white label, No. 8. M.K. VII containing 32 grs. fulminate of mercury.

COMMERCIAL (Long)

COMMERCIAL (Short)

Description. Copper tube, open one end, containing 25 grs. fulminate of mercury. [Pg 57]

### EXPLODERS

SERVICE

Guncotton. One-oz. primer, 15-oz. slab. See Explosives, Guncotton.

No. 2 Detonator for Hand Grenade. Consists of brass tube (detonator holder) with flat screw head. The other end is fitted with a cavity which carries N.G. percussion cap. A commercial detonator open end toward the screw head is placed inside, its open end closed with a wooden plug; the closed end is pierced with four flash holes to enable flash from percussion cap to communicate with F. of M. in detonator. A brass screw in head of detonator holder closes detonator tube.

This detonator has three screw threads.

No. 3 Detonator. See description of No. 2. This detonator is ¼ in. longer than No. 2, and has two screw threads.

### PATENT LIGHTERS

Nobel Lighter. (See Plates 8 and 9.) The lighter is made up of two cardboard tubes, one fitting over the other; inside the end of the larger tube is a small brass cap containing friction composition. At the top of the smaller tube are two friction points. These points are held about ¼ in. from the cap containing friction composition, by a safety pin passing through both tubes. At the other end of the smaller tube is a small copper band into which the fuse can be crimped. A narrow band of waterproof tape with a loose end is glued around the joint of the two tubes to keep out moisture. [Pg 58]

To Assemble. Insert fuse into lighter, fasten by crimping, and insert other end of fuse into detonator. The joints at lighter and detonator should be waxed to make it damp-proof and flash-proof.

Brock Lighter. See Grenade Hand. Consists of a small cardboard cup filled with friction composition, covered with waterproof paper. The latter can be torn off by pulling a small tag which is left free.

Grenades with fuses are so arranged (with sufficient length of fuse) to explode from 3 to 5 seconds after being ignited and thrown, giving the thrower plenty of time (when throwing from a trench) to bend down safe. Grenades, without fuses (but with detonators only) will explode on impact; for instance, in Grenade No. 1, Mark I, it is obvious when instructions (see p. 2, Grenade 1) are carried out, and grenade is thrown, that the steel needle will be driven into the detonator and exploded.

In Grenade No. 3, Mark I, when safety pin is removed and releasing socket slipped back, the wind vane revolves backward (during the passage through the air) until far enough to allow the retaining bolt to fall out. This leaves nothing between the firing needle and detonator cap except a very thin spiral spring which is only strong enough to hold the weight of the needle pellet until the shock of impact when the grenade explodes.

In Grenade No. 20 releasing collar slips back on the rifle being fired.

In Grenade No. 5, Mark I. On this grenade being thrown the pressure of the fingers being released the striking lever flies outward by the pressure of the powerful spring, releasing the shoulder of the firing striker which is driven on to the fuse and explodes in 4½ seconds.

All other grenades, see pages opposite plates.

[Pg 59]

## THROWING

Hand grenades are held firmly in the hand behind the thrower, the arm is brought quickly upward with a sweeping movement (the arm straight all the time), the grenade will be let go when the hand is above the thrower’s head, and should describe a semicircle in its flight.

Hand grenades can be thrown from 30 to 50 yards, rifle grenades from 200 to 400 yards.

Attacks should be practiced with dummy and deteriorated grenades, i.e., grenades with only a detonator and no explosive, etc.

Confidence and knowledge of grenades should be gained by students handling, stripping and assembling all types and handling fuses and detonators, as often as possible.

The importance of grenade work cannot be over-estimated and one can imagine numberless cases when a grenade is more useful than any other weapon. For instance, in street fighting a number of the enemy are holding a house and firing from an upper window commanding the main approach. You cannot get at them with a rifle, but it might be comparatively easy for one or two men to get along to the house by back ways, using the other houses for shelter and throw a grenade through the window, killing everyone in the room.

Transcriber’s Notes:

The cover is in the public domain.

The illustrations have been moved so that they do not break up paragraphs and so that they are next to the text they illustrate.

Typographical errors have been silently corrected but other variations in spelling and punctuation remain unaltered.

    End of the Project Gutenberg EBook of Hand Grenades, by Graham M. Ainslie

    *** END OF THIS PROJECT GUTENBERG EBOOK HAND GRENADES ***

    ***** This file should be named 56638-h.htm or 56638-h.zip *****
    This and all associated files of various formats will be found in:
            http://www.gutenberg.org/5/6/6/3/56638/

    Produced by Chris Curnow, Paul Marshall and the Online
    Distributed Proofreading Team at http://www.pgdp.net (This
    file was produced from images generously made available
    by The Internet Archive)

    Updated editions will replace the previous one--the old editions will
    be renamed.

    Creating the works from print editions not protected by U.S. copyright
    law means that no one owns a United States copyright in these works,
    so the Foundation (and you!) can copy and distribute it in the United
    States without permission and without paying copyright
    royalties. Special rules, set forth in the General Terms of Use part
    of this license, apply to copying and distributing Project
    Gutenberg-tm electronic works to protect the PROJECT GUTENBERG-tm
    concept and trademark. Project Gutenberg is a registered trademark,
    and may not be used if you charge for the eBooks, unless you receive
    specific permission. If you do not charge anything for copies of this
    eBook, complying with the rules is very easy. You may use this eBook
    for nearly any purpose such as creation of derivative works, reports,
    performances and research. They may be modified and printed and given
    away--you may do practically ANYTHING in the United States with eBooks
    not protected by U.S. copyright law. Redistribution is subject to the
    trademark license, especially commercial redistribution.

    START: FULL LICENSE

    THE FULL PROJECT GUTENBERG LICENSE
    PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK

    To protect the Project Gutenberg-tm mission of promoting the free
    distribution of electronic works, by using or distributing this work
    (or any other work associated in any way with the phrase "Project
    Gutenberg"), you agree to comply with all the terms of the Full
    Project Gutenberg-tm License available with this file or online at
    www.gutenberg.org/license.

    Section 1. General Terms of Use and Redistributing Project
    Gutenberg-tm electronic works

    1.A. By reading or using any part of this Project Gutenberg-tm
    electronic work, you indicate that you have read, understand, agree to
    and accept all the terms of this license and intellectual property
    (trademark/copyright) agreement. If you do not agree to abide by all
    the terms of this agreement, you must cease using and return or
    destroy all copies of Project Gutenberg-tm electronic works in your
    possession. If you paid a fee for obtaining a copy of or access to a
    Project Gutenberg-tm electronic work and you do not agree to be bound
    by the terms of this agreement, you may obtain a refund from the
    person or entity to whom you paid the fee as set forth in paragraph
    1.E.8.

    1.B. "Project Gutenberg" is a registered trademark. It may only be
    used on or associated in any way with an electronic work by people who
    agree to be bound by the terms of this agreement. There are a few
    things that you can do with most Project Gutenberg-tm electronic works
    even without complying with the full terms of this agreement. See
    paragraph 1.C below. There are a lot of things you can do with Project
    Gutenberg-tm electronic works if you follow the terms of this
    agreement and help preserve free future access to Project Gutenberg-tm
    electronic works. See paragraph 1.E below.

    1.C. The Project Gutenberg Literary Archive Foundation ("the
    Foundation" or PGLAF), owns a compilation copyright in the collection
    of Project Gutenberg-tm electronic works. Nearly all the individual
    works in the collection are in the public domain in the United
    States. If an individual work is unprotected by copyright law in the
    United States and you are located in the United States, we do not
    claim a right to prevent you from copying, distributing, performing,
    displaying or creating derivative works based on the work as long as
    all references to Project Gutenberg are removed. Of course, we hope
    that you will support the Project Gutenberg-tm mission of promoting
    free access to electronic works by freely sharing Project Gutenberg-tm
    works in compliance with the terms of this agreement for keeping the
    Project Gutenberg-tm name associated with the work. You can easily
    comply with the terms of this agreement by keeping this work in the
    same format with its attached full Project Gutenberg-tm License when
    you share it without charge with others.

    1.D. The copyright laws of the place where you are located also govern
    what you can do with this work. Copyright laws in most countries are
    in a constant state of change. If you are outside the United States,
    check the laws of your country in addition to the terms of this
    agreement before downloading, copying, displaying, performing,
    distributing or creating derivative works based on this work or any
    other Project Gutenberg-tm work. The Foundation makes no
    representations concerning the copyright status of any work in any
    country outside the United States.

    1.E. Unless you have removed all references to Project Gutenberg:

    1.E.1. The following sentence, with active links to, or other
    immediate access to, the full Project Gutenberg-tm License must appear
    prominently whenever any copy of a Project Gutenberg-tm work (any work
    on which the phrase "Project Gutenberg" appears, or with which the
    phrase "Project Gutenberg" is associated) is accessed, displayed,
    performed, viewed, copied or distributed:

      This eBook is for the use of anyone anywhere in the United States and
      most other parts of the world at no cost and with almost no
      restrictions whatsoever. You may copy it, give it away or re-use it
      under the terms of the Project Gutenberg License included with this
      eBook or online at www.gutenberg.org. If you are not located in the
      United States, you'll have to check the laws of the country where you
      are located before using this ebook.

    1.E.2. If an individual Project Gutenberg-tm electronic work is
    derived from texts not protected by U.S. copyright law (does not
    contain a notice indicating that it is posted with permission of the
    copyright holder), the work can be copied and distributed to anyone in
    the United States without paying any fees or charges. If you are
    redistributing or providing access to a work with the phrase "Project
    Gutenberg" associated with or appearing on the work, you must comply
    either with the requirements of paragraphs 1.E.1 through 1.E.7 or
    obtain permission for the use of the work and the Project Gutenberg-tm
    trademark as set forth in paragraphs 1.E.8 or 1.E.9.

    1.E.3. If an individual Project Gutenberg-tm electronic work is posted
    with the permission of the copyright holder, your use and distribution
    must comply with both paragraphs 1.E.1 through 1.E.7 and any
    additional terms imposed by the copyright holder. Additional terms
    will be linked to the Project Gutenberg-tm License for all works
    posted with the permission of the copyright holder found at the
    beginning of this work.

    1.E.4. Do not unlink or detach or remove the full Project Gutenberg-tm
    License terms from this work, or any files containing a part of this
    work or any other work associated with Project Gutenberg-tm.

    1.E.5. Do not copy, display, perform, distribute or redistribute this
    electronic work, or any part of this electronic work, without
    prominently displaying the sentence set forth in paragraph 1.E.1 with
    active links or immediate access to the full terms of the Project
    Gutenberg-tm License.

    1.E.6. You may convert to and distribute this work in any binary,
    compressed, marked up, nonproprietary or proprietary form, including
    any word processing or hypertext form. However, if you provide access
    to or distribute copies of a Project Gutenberg-tm work in a format
    other than "Plain Vanilla ASCII" or other format used in the official
    version posted on the official Project Gutenberg-tm web site
    (www.gutenberg.org), you must, at no additional cost, fee or expense
    to the user, provide a copy, a means of exporting a copy, or a means
    of obtaining a copy upon request, of the work in its original "Plain
    Vanilla ASCII" or other form. Any alternate format must include the
    full Project Gutenberg-tm License as specified in paragraph 1.E.1.

    1.E.7. Do not charge a fee for access to, viewing, displaying,
    performing, copying or distributing any Project Gutenberg-tm works
    unless you comply with paragraph 1.E.8 or 1.E.9.

    1.E.8. You may charge a reasonable fee for copies of or providing
    access to or distributing Project Gutenberg-tm electronic works
    provided that

    * You pay a royalty fee of 20% of the gross profits you derive from
      the use of Project Gutenberg-tm works calculated using the method
      you already use to calculate your applicable taxes. The fee is owed
      to the owner of the Project Gutenberg-tm trademark, but he has
      agreed to donate royalties under this paragraph to the Project
      Gutenberg Literary Archive Foundation. Royalty payments must be paid
      within 60 days following each date on which you prepare (or are
      legally required to prepare) your periodic tax returns. Royalty
      payments should be clearly marked as such and sent to the Project
      Gutenberg Literary Archive Foundation at the address specified in
      Section 4, "Information about donations to the Project Gutenberg
      Literary Archive Foundation."

    * You provide a full refund of any money paid by a user who notifies
      you in writing (or by e-mail) within 30 days of receipt that s/he
      does not agree to the terms of the full Project Gutenberg-tm
      License. You must require such a user to return or destroy all
      copies of the works possessed in a physical medium and discontinue
      all use of and all access to other copies of Project Gutenberg-tm
      works.

    * You provide, in accordance with paragraph 1.F.3, a full refund of
      any money paid for a work or a replacement copy, if a defect in the
      electronic work is discovered and reported to you within 90 days of
      receipt of the work.

    * You comply with all other terms of this agreement for free
      distribution of Project Gutenberg-tm works.

    1.E.9. If you wish to charge a fee or distribute a Project
    Gutenberg-tm electronic work or group of works on different terms than
    are set forth in this agreement, you must obtain permission in writing
    from both the Project Gutenberg Literary Archive Foundation and The
    Project Gutenberg Trademark LLC, the owner of the Project Gutenberg-tm
    trademark. Contact the Foundation as set forth in Section 3 below.

    1.F.

    1.F.1. Project Gutenberg volunteers and employees expend considerable
    effort to identify, do copyright research on, transcribe and proofread
    works not protected by U.S. copyright law in creating the Project
    Gutenberg-tm collection. Despite these efforts, Project Gutenberg-tm
    electronic works, and the medium on which they may be stored, may
    contain "Defects," such as, but not limited to, incomplete, inaccurate
    or corrupt data, transcription errors, a copyright or other
    intellectual property infringement, a defective or damaged disk or
    other medium, a computer virus, or computer codes that damage or
    cannot be read by your equipment.

    1.F.2. LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the "Right
    of Replacement or Refund" described in paragraph 1.F.3, the Project
    Gutenberg Literary Archive Foundation, the owner of the Project
    Gutenberg-tm trademark, and any other party distributing a Project
    Gutenberg-tm electronic work under this agreement, disclaim all
    liability to you for damages, costs and expenses, including legal
    fees. YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT
    LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE
    PROVIDED IN PARAGRAPH 1.F.3. YOU AGREE THAT THE FOUNDATION, THE
    TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE
    LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR
    INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH
    DAMAGE.

    1.F.3. LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a
    defect in this electronic work within 90 days of receiving it, you can
    receive a refund of the money (if any) you paid for it by sending a
    written explanation to the person you received the work from. If you
    received the work on a physical medium, you must return the medium
    with your written explanation. The person or entity that provided you
    with the defective work may elect to provide a replacement copy in
    lieu of a refund. If you received the work electronically, the person
    or entity providing it to you may choose to give you a second
    opportunity to receive the work electronically in lieu of a refund. If
    the second copy is also defective, you may demand a refund in writing
    without further opportunities to fix the problem.

    1.F.4. Except for the limited right of replacement or refund set forth
    in paragraph 1.F.3, this work is provided to you 'AS-IS', WITH NO
    OTHER WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT
    LIMITED TO WARRANTIES OF MERCHANTABILITY OR FITNESS FOR ANY PURPOSE.

    1.F.5. Some states do not allow disclaimers of certain implied
    warranties or the exclusion or limitation of certain types of
    damages. If any disclaimer or limitation set forth in this agreement
    violates the law of the state applicable to this agreement, the
    agreement shall be interpreted to make the maximum disclaimer or
    limitation permitted by the applicable state law. The invalidity or
    unenforceability of any provision of this agreement shall not void the
    remaining provisions.

    1.F.6. INDEMNITY - You agree to indemnify and hold the Foundation, the
    trademark owner, any agent or employee of the Foundation, anyone
    providing copies of Project Gutenberg-tm electronic works in
    accordance with this agreement, and any volunteers associated with the
    production, promotion and distribution of Project Gutenberg-tm
    electronic works, harmless from all liability, costs and expenses,
    including legal fees, that arise directly or indirectly from any of
    the following which you do or cause to occur: (a) distribution of this
    or any Project Gutenberg-tm work, (b) alteration, modification, or
    additions or deletions to any Project Gutenberg-tm work, and (c) any
    Defect you cause.

    Section 2. Information about the Mission of Project Gutenberg-tm

    Project Gutenberg-tm is synonymous with the free distribution of
    electronic works in formats readable by the widest variety of
    computers including obsolete, old, middle-aged and new computers. It
    exists because of the efforts of hundreds of volunteers and donations
    from people in all walks of life.

    Volunteers and financial support to provide volunteers with the
    assistance they need are critical to reaching Project Gutenberg-tm's
    goals and ensuring that the Project Gutenberg-tm collection will
    remain freely available for generations to come. In 2001, the Project
    Gutenberg Literary Archive Foundation was created to provide a secure
    and permanent future for Project Gutenberg-tm and future
    generations. To learn more about the Project Gutenberg Literary
    Archive Foundation and how your efforts and donations can help, see
    Sections 3 and 4 and the Foundation information page at
    www.gutenberg.org

    Section 3. Information about the Project Gutenberg Literary Archive Foundation

    The Project Gutenberg Literary Archive Foundation is a non profit
    501(c)(3) educational corporation organized under the laws of the
    state of Mississippi and granted tax exempt status by the Internal
    Revenue Service. The Foundation's EIN or federal tax identification
    number is 64-6221541. Contributions to the Project Gutenberg Literary
    Archive Foundation are tax deductible to the full extent permitted by
    U.S. federal laws and your state's laws.

    The Foundation's principal office is in Fairbanks, Alaska, with the
    mailing address: PO Box 750175, Fairbanks, AK 99775, but its
    volunteers and employees are scattered throughout numerous
    locations. Its business office is located at 809 North 1500 West, Salt
    Lake City, UT 84116, (801) 596-1887. Email contact links and up to
    date contact information can be found at the Foundation's web site and
    official page at www.gutenberg.org/contact

    For additional contact information:

        Dr. Gregory B. Newby
        Chief Executive and Director
        gbnewby@pglaf.org

    Section 4. Information about Donations to the Project Gutenberg
    Literary Archive Foundation

    Project Gutenberg-tm depends upon and cannot survive without wide
    spread public support and donations to carry out its mission of
    increasing the number of public domain and licensed works that can be
    freely distributed in machine readable form accessible by the widest
    array of equipment including outdated equipment. Many small donations
    ($1 to $5,000) are particularly important to maintaining tax exempt
    status with the IRS.

    The Foundation is committed to complying with the laws regulating
    charities and charitable donations in all 50 states of the United
    States. Compliance requirements are not uniform and it takes a
    considerable effort, much paperwork and many fees to meet and keep up
    with these requirements. We do not solicit donations in locations
    where we have not received written confirmation of compliance. To SEND
    DONATIONS or determine the status of compliance for any particular
    state visit www.gutenberg.org/donate

    While we cannot and do not solicit contributions from states where we
    have not met the solicitation requirements, we know of no prohibition
    against accepting unsolicited donations from donors in such states who
    approach us with offers to donate.

    International donations are gratefully accepted, but we cannot make
    any statements concerning tax treatment of donations received from
    outside the United States. U.S. laws alone swamp our small staff.

    Please check the Project Gutenberg Web pages for current donation
    methods and addresses. Donations are accepted in a number of other
    ways including checks, online payments and credit card donations. To
    donate, please visit: www.gutenberg.org/donate

    Section 5. General Information About Project Gutenberg-tm electronic works.

    Professor Michael S. Hart was the originator of the Project
    Gutenberg-tm concept of a library of electronic works that could be
    freely shared with anyone. For forty years, he produced and
    distributed Project Gutenberg-tm eBooks with only a loose network of
    volunteer support.

    Project Gutenberg-tm eBooks are often created from several printed
    editions, all of which are confirmed as not protected by copyright in
    the U.S. unless a copyright notice is included. Thus, we do not
    necessarily keep eBooks in compliance with any particular paper
    edition.

    Most people start at our Web site which has the main PG search
    facility: www.gutenberg.org

    This Web site includes information about Project Gutenberg-tm,
    including how to make donations to the Project Gutenberg Literary
    Archive Foundation, how to help produce our new eBooks, and how to
    subscribe to our email newsletter to hear about new eBooks.